mqtt:
  # The MQTT broker to connect to
  server: tcp://127.0.0.1:1883
  # Optional: Username and Password for authenticating with the MQTT Server
  # user: bob
  # password: happylittleclouds
  # Optional: for TLS client certificates
  # ca_cert: certs/AmazonRootCA1.pem
  # client_cert: certs/xxxxx-certificate.pem.crt
  # client_key: certs/xxxxx-private.pem.key
  # Optional: Used to specify ClientID. The default is <hostname>-<pid>
  # client_id: somedevice
  # The Topic path to subscribe to. Be aware that you have to specify the wildcard.
  topic_path: v1/devices/me/+
  # Optional: Regular expression to extract the device ID from the topic path. The default regular expression, assumes
  # that the last "element" of the topic_path is the device id.
  # The regular expression must contain a named capture group with the name deviceid
  # For example the expression for tasamota based sensors is "tele/(?P<deviceid>.*)/.*"
  # device_id_regex: "(.*/)?(?P<deviceid>.*)"
  # The MQTT QoS level
  qos: 0
# Export internal profiling metrics including CPU, Memory, uptime, open file
# descriptors, as well as metrics exported by Go runtime such as information about
# heap and garbage collection stats.
enable_profiling_metrics: false
cache:
  # Timeout. Each received metric will be presented for this time if no update is send via MQTT.
  # Set the timeout to -1 to disable the deletion of metrics from the cache. The exporter presents the ingest timestamp
  # to prometheus.
  timeout: 24h
json_parsing:
  # Separator. Used to split path to elements when accessing json fields.
  # You can access json fields with dots in it. F.E. {"key.name": {"nested": "value"}}
  # Just set separator to -> and use key.name->nested as mqtt_name
  separator: .
# This is a list of valid metrics. Only metrics listed here will be exported
metrics:
    # The name of the metric in prometheus
  - prom_name: temperature
    # The name of the metric in a MQTT JSON message
    mqtt_name: temperature
    # The prometheus help text for this metric
    help: DHT22 temperature reading
    # The prometheus type for this metric. Valid values are: "gauge" and "counter"
    type: gauge
    # A map of string to string for constant labels. This labels will be attached to every prometheus metric
    const_labels:
      sensor_type: dht22
    # The name of the metric in prometheus
  - prom_name: humidity
    # The name of the metric in a MQTT JSON message
    mqtt_name: humidity
    # The prometheus help text for this metric
    help: DHT22 humidity reading
    # The prometheus type for this metric. Valid values are: "gauge" and "counter"
    type: gauge
    # A map of string to string for constant labels. This labels will be attached to every prometheus metric
    const_labels:
      sensor_type: dht22
    # The name of the metric in prometheus
  - prom_name: heat_index
    # The name of the metric in a MQTT JSON message
    mqtt_name: heat_index
    # The prometheus help text for this metric
    help: DHT22 heatIndex calculation
    # The prometheus type for this metric. Valid values are: "gauge" and "counter"
    type: gauge
    # A map of string to string for constant labels. This labels will be attached to every prometheus metric
    const_labels:
      sensor_type: dht22
    # The name of the metric in prometheus
  - prom_name: state
    # The name of the metric in a MQTT JSON message
    mqtt_name: state
    # Regular expression to only match sensors with the given name pattern
    sensor_name_filter: "^.*-light$"
    # The prometheus help text for this metric
    help: Light state
    # The prometheus type for this metric. Valid values are: "gauge" and "counter"
    type: gauge
    # A map of string to string for constant labels. This labels will be attached to every prometheus metric
    const_labels:
      sensor_type: ikea
    # Metric value to use if a value cannot be parsed (match cannot be found in the map above, invalid float parsing, ...)
    # If not specified, parsing error will occur.
    error_value: 1
    # When specified, enables mapping between string values to metric values.
    string_value_mapping:
      # A map of string to metric value.
      map:
        off: 0
        low: 0
